,Nominal Cooling Capacity (Tons)##other##,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Description##other##,Series##other##,Model##other##,Overall Depth##length##inches,Overall Height##length##inches,Overall Width##length##inches,System Performance HSPF2##other##,SEER2##other##,Unit Weight##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Minimum Circuit Amps##electrical_current##amperes,Frequency##electrical_frequency##hertz,Phase##other##,Voltage##electrical_potential##volts,Voltage Comments##other##,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Compressor Rated Load Amps##electrical_current##amperes,Compressor Type##other##,Refrigerant Charge##force##pounds_force,Refrigerant Used##other##,Back Clearance##length##inches,Base Mounts Center Offset##length##inches,Enclosure Depth##length##inches,Front Clearance##length##inches,Left Clearance##length##inches,Outside Fan Diameter##length##inches,Right Clearance##length##inches,Top Clearance##length##inches,Refrigerant Horizontal Offset##length##inches,Refrigerant Liquid Vertical Offset##length##inches,Refrigerant Suction Gas Vertical Offset##length##inches,Standards##other##,Product Page URL##other##,URL##other##
2Ton_Single_Fan_7SCP18V24P-01A,2,24000,Cold Climate Variable Capacity Side Discharge Heat Pump,7SCP18V,7SCP18V24P-01A,17 1/8,30,40 1/4,10,18,137,30,21,60,1,230,208 VAC - 230 VAC, 3/8,0.750,14.500,Variable Frequency Rotary,3.56,R-454B,12,13,15.75,40,4,22,4,40,3.72,5.16,2.36,"AHRI 210/240-2023, UL, ETL, ENERGY STAR",https://www.allied-commercial.com/,https://www.allied-commercial.com/
3Ton_Single_Fan_7SCP18V36P-01A,3,36000,Cold Climate Variable Capacity Side Discharge Heat Pump,7SCP18V,7SCP18V36P-01A,19 7/8,33 1/8,43 1/8,10,18,157,35,24,60,1,230,208 VAC - 230 VAC, 3/8,0.875,16.500,Variable Frequency Rotary,5.56,R-454B,12,14.75,17,40,4,25,4,40,3.72,5.16,2.36,"AHRI 210/240-2023, UL, ETL, ENERGY STAR",https://www.allied-commercial.com/,https://www.allied-commercial.com/
4Ton_Double_Fan_7SCP18V60P-01A,4,48000,Cold Climate Variable Capacity Side Discharge Heat Pump,7SCP18V,7SCP18V60P-01A,19 7/8,45 3/8,41 5/8,10,18,245,60,37,60,1,230,208 VAC - 230 VAC, 3/8,0.875,26.400,Variable Frequency Rotary,7.5,R-454B,12,14.75,17,40,4,20,4,40,3.72,5.16,2.36,"AHRI 210/240-2023, UL, ETL, ENERGY STAR",https://www.allied-commercial.com/,https://www.allied-commercial.com/
5Ton_Double_Fan_7SCP18V60P-01A,5,60000,Cold Climate Variable Capacity Side Discharge Heat Pump,7SCP18V,7SCP18V60P-01A,19 7/8,45 3/8,41 5/8,10,18,245,60,37,60,1,230,208 VAC - 230 VAC, 3/8,0.875,26.400,Variable Frequency Rotary,7.5,R-454B,12,14.75,17,40,4,20,4,40,3.72,5.16,2.36,"AHRI 210/240-2023, UL, ETL, ENERGY STAR",https://www.allied-commercial.com/,https://www.allied-commercial.com/