,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Compressor Locked Rotor Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
1.5Ton_7AC13F18P-**A,18000,24.5,24.25,24.25,7AC13F,7AC13F18P-**A,11.1,1.5,128,Air Conditioner,73.0,1,60,230 VAC,230, 3/8,0.75,4.5625,15.0,8.3,45.0,R-454B,4,7,25.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
2Ton_7AC13F24P-**A,24000,28.5,24.25,24.25,7AC13F,7AC13F24P-**A,13.5,2.0,134,Air Conditioner,76.0,1,60,230 VAC,230, 3/8,0.75,5.0,20.0,10.2,60.2,R-454B,4,7,29.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
2.5Ton_7AC13F30P-**A,30000,28.5,28.25,28.25,7AC13F,7AC13F30P-**A,16.6,2.5,152,Air Conditioner,76.0,1,60,230 VAC,230, 3/8,0.75,5.4375,25.0,12.5,67.8,R-454B,4,7,29.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_7AC13F36P-**A,36000,32.5,28.25,28.25,7AC13F,7AC13F36P-**A,17.8,3.0,161,Air Conditioner,76.0,1,60,230 VAC,230, 3/8,0.875,6.1875,30.0,13.4,82.5,R-454B,4,7,33.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_7AC13F42P-**A,42000,36.5,28.25,28.25,7AC13F,7AC13F42P-**A,21.2,3.5,195,Air Conditioner,76.0,1,60,230 VAC,230, 3/8,0.875,6.6875,35.0,14.9,109.0,R-454B,4,7,37.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_7AC13F48P-**A,48000,28.5,28.25,28.25,7AC13F,7AC13F48P-**A,24.3,4.0,215,Air Conditioner,78.0,1,60,230 VAC,230, 3/8,0.875,8.1875,40.0,18.0,126.0,R-454B,4,7,29.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_7AC13F60P-**A,60000,36.5,28.25,28.25,7AC13F,7AC13F60P-**A,31.3,5.0,250,Air Conditioner,80.0,1,60,230 VAC,230, 3/8,1.125,9.0625,50.0,23.7,157.0,R-454B,4,7,37.25,2.0,4.375,6.375,2.0,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,7AC13F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System