,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
2Ton_A7HP19V36P-**A,24000,33.0,29.375,31.25,A7HP19V,A7HP19V36P-**A,23.0,2.0,215,Heat Pump,70,1,60,230 VAC,230, 3/8,0.75,8.5,35,16.3,R-454B,4,7,33.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/heat-pumps,A7HP19V,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_A7HP19V36P-**A,36000,33.0,29.375,31.25,A7HP19V,A7HP19V36P-**A,23.0,3.0,215,Heat Pump,76,1,60,230 VAC,230, 3/8,0.875,8.5,35,16.3,R-454B,4,7,33.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/heat-pumps,A7HP19V,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_A7HP19V60P-**A,48000,43.0,29.375,31.25,A7HP19V,A7HP19V60P-**A,39.2,4.0,272,Heat Pump,72,1,60,230 VAC,230, 3/8,0.875,9.375,60,28.5,R-454B,4,7,43.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/heat-pumps,A7HP19V,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_A7HP19V60P-**A,60000,43.0,29.375,31.25,A7HP19V,A7HP19V60P-**A,39.2,5.0,272,Heat Pump,78,1,60,230 VAC,230, 3/8,1.25,9.375,60,28.5,R-454B,4,7,43.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/heat-pumps,A7HP19V,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System