,Nominal Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Enclosure Height##length##inches,Overall Width##length##inches,Overall Depth##length##inches,Model##other##,Model Number##other##,Minimum Circuit Amps##electrical_current##amperes,Nominal Cooling Capacity (Tons)##other##,Unit Weight##force##pounds_force,Description##other##,Sound Pressure Level_dBA##other##,Phase##other##,Frequency##electrical_frequency##hertz,Voltage Comments##other##,Voltage##electrical_potential##volts,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Suction Gas Connection Diameter##pipe_size##inches,Refrigerant Charge##force##pounds_force,Maximum Overcurrent Protection##electrical_current##amperes,Compressor Rated Load Amps##electrical_current##amperes,Compressor Locked Rotor Amps##electrical_current##amperes,Refrigerant Used##other##,Lower Access Panel Depth##length##inches,Lower Access Panel Width##length##inches,Base Unit Height##length##inches,Standoff Height##length##inches,Standoff Offset A##length##inches,Standoff Offset B##length##inches,Suction Valve Height##length##inches,Clearance Length##length##inches,Enclosure Material##other##,URL##other##,Product Page URL##other##,Series##other##,Standards##other##
1.5Ton_A7AC14F18P-**A,18000,29.0,29.375,31.25,A7AC14F,A7AC14F18P-**A,11.2,1.5,170,Air Conditioner,76,1,60,230 VAC,230, 3/8,0.75,5.4375,15,8.3,45.0,R-454B,4,7,29.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
2Ton_A7AC14F24P-**A,24000,37.0,29.375,31.25,A7AC14F,A7AC14F24P-**A,13.6,2.0,190,Air Conditioner,75,1,60,230 VAC,230, 3/8,0.75,5.4375,20,10.3,60.2,R-454B,4,7,37.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
2.5Ton_A7AC14F30P-**A,30000,29.0,29.375,31.25,A7AC14F,A7AC14F30P-**A,16.6,2.5,190,Air Conditioner,72,1,60,230 VAC,230, 3/8,0.75,6.1875,25,12.7,75.6,R-454B,4,7,29.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3Ton_A7AC14F36P-**A,36000,37.0,29.375,31.25,A7AC14F,A7AC14F36P-**A,21.8,3.0,220,Air Conditioner,73,1,60,230 VAC,230, 3/8,0.875,7.375,30,16.7,93.5,R-454B,4,7,37.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_A7AC14F41P-**A,42000,33.0,35.75,37.75,A7AC14F,A7AC14F41P-**A,21.0,3.5,270,Air Conditioner,74,1,60,230 VAC,230, 3/8,0.875,8.0,35,14.7,109.0,R-454B,4,7,33.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
3.5Ton_A7AC14F42P-**A,42000,33.0,35.75,37.75,A7AC14F,A7AC14F42P-**A,23.2,3.5,250,Air Conditioner,76,1,60,230 VAC,230, 3/8,0.875,7.6875,35,17.3,123.0,R-454B,4,7,33.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_A7AC14F47P-**A,48000,33.0,35.75,37.75,A7AC14F,A7AC14F47P-**A,25.2,4.0,270,Air Conditioner,74,1,60,230 VAC,230, 3/8,1.875,8.375,35,18.1,126.0,R-454B,4,7,33.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
4Ton_A7AC14F48P-**A,48000,43.0,29.375,31.25,A7AC14F,A7AC14F48P-**A,29.7,4.0,260,Air Conditioner,75,1,60,230 VAC,230, 3/8,0.875,9.4375,50,22.4,126.0,R-454B,4,7,43.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_A7AC14F59P-**A,60000,43.0,35.75,37.75,A7AC14F,A7AC14F59P-**A,31.8,5.0,300,Air Conditioner,73,1,60,230 VAC,230, 3/8,0.875,10.0625,50,23.3,143.0,R-454B,4,7,43.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System
5Ton_A7AC14F60P-**A,60000,43.0,35.75,37.75,A7AC14F,A7AC14F60P-**A,31.2,5.0,305,Air Conditioner,75,1,60,230 VAC,230, 3/8,1.125,9.4375,50,23.7,157.0,R-454B,4,7,43.75,2,4.375,6.375,2,36,Metal - Allied Air - Steel - Warm Gray,https://www.allied-commercial.com/,https://www.alliednow.com/products/air-conditioners,A7AC14F,AHRI Standard 210/240/270 certified; ETL certified; ISO 9001 Registered Manufacturing Quality System